[SemImageFile]
InstructName=SU8200
SemVersion=03-21
SDMVersion=
SerialNumber=8200-16D2-05
DataNumber=NFL-Ro 0001
SampleName=
Format=tif
ImageName=Al-Ta_2.5kx.tif
Directory=D:\2026\EuroLabs\
Date=05/13/2026
Time=13:28:24
Media=HD[Data]
DataSize=2560x1920
PixelSize=19.84375
SignalName=SE(U)
DisplaySignalName=SE(U)
SEDetSetting=
AcceleratingVoltage=10000 Volt
DecelerationVoltage=0 Volt
DecelerationMode=
Magnification=2500
WorkingDistance=5658.94 um
EmissionCurrent=9000 nA
LensMode=Normal
PhotoSize=1000
MagnificationDisplay=0
Vacuum=
MicronMarker=20000
SubMagnification=0
SubSignalName=
SpecimenBias=0 V
Condencer1=5000
ScanSpeed=Capture_Slow(40)
CaptureSpeed_Integration=
CalibrationScanSpeed=24
ImgEnhance=0
ColorMode=Grayscale
ColorPalette=
ScreenMode=Middle Screen
Comment=
KeyWord1=
KeyWord2=
Condition=Vacc=10.0kV   Mag=x2.50k   WD=5.7mm
DataDisplayCombine=1
StageType=5
StagePositionX=35077000
StagePositionY=55055000
StagePositionR=0
StagePositionZ=5000000
StagePositionT=0
FocusDepth=1.0
DynamicFocus=0
TiltCompensation=0
RasterRotation=0.0
MagneticSample=OFF
EBIC_Value00=
EBIC_ValueFF=
EBIC_Polarity=
DriftCorrectionIntegration=0
LiveImgEnhance=0
