[SemImageFile]
InstructName=SU8200
SemVersion=03-21
SDMVersion=
SerialNumber=8200-16D2-05
DataNumber=NFL-Ro 0001
SampleName=
Format=tif
ImageName=Al-Ta_70kx.tif
Directory=D:\2026\EuroLabs\01_13May2026_Red\
Date=05/13/2026
Time=13:35:07
Media=HD[Data]
DataSize=1280x960
PixelSize=1.417411
SignalName=SE(U)
DisplaySignalName=SE(U)
SEDetSetting=
AcceleratingVoltage=10000 Volt
DecelerationVoltage=0 Volt
DecelerationMode=
Magnification=70000
WorkingDistance=5659.04 um
EmissionCurrent=9400 nA
LensMode=Normal
PhotoSize=1000
MagnificationDisplay=0
Vacuum=
MicronMarker=500
SubMagnification=0
SubSignalName=
SpecimenBias=0 V
Condencer1=5000
ScanSpeed=Capture_Rapid(32)
CaptureSpeed_Integration=
CalibrationScanSpeed=19
ImgEnhance=0
ColorMode=Grayscale
ColorPalette=
ScreenMode=Middle Screen
Comment=
KeyWord1=
KeyWord2=
Condition=Vacc=10.0kV   Mag=x70.0k   WD=5.7mm
DataDisplayCombine=1
StageType=5
StagePositionX=35078999
StagePositionY=55058998
StagePositionR=0
StagePositionZ=5000000
StagePositionT=0
FocusDepth=1.0
DynamicFocus=0
TiltCompensation=0
RasterRotation=0.0
MagneticSample=OFF
EBIC_Value00=
EBIC_ValueFF=
EBIC_Polarity=
DriftCorrectionIntegration=1
LiveImgEnhance=0
